;*************************************************************************
;
;Copyright 2000-2009 3M. All rights reserved.
;
;Module Name: 	TwTouch.INF
;
;Abstract:	INF file installs MicroTouch Touch Screen driver
;
;*************************************************************************

[Version]
Signature="$WINDOWS NT$"
Class=Mouse
ClassGUID={4D36E96F-E325-11CE-BFC1-08002BE10318}
Provider=%MMM%
DriverVer=01/09/2009, 7.12.6.0
CatalogFile=TwTouch.cat

[SourceDisksNames]
1 = %DiskId1%,,,

[DestinationDirs]
DefaultDestDir=12

[SourceDisksFiles]
TwTouch.sys   = 1,,

; ***********************************************************************
[Manufacturer]
%StdMfg%=Standard,NTamd64

[Standard]

;* This is the pseudo device used by the non-PnP serial bus driver *
%TwTouch.DeviceDescSerial%=TwTouch_Device,      PnP\TwTouch           ;Non-PnP Serial

;* These hardware IDs are for the EX II USB controllers *
%TwTouch.DeviceDescEXIIUSB%=TwTouch_Device,     USB\VID_0596&PID_0001 ;USB EXII
%TwTouch.DeviceDescEXIIUSBRom%=TwTouch_Device,  USB\VID_0596&PID_0002 ;USB EXII fix code
%TwTouch.DeviceDescEXIIHID%=TwTouch_Device,     USB\VID_0596&PID_0003 ;USB EXII HID

;* These hardware IDs are for the serial PnP controllers *
%TwTouch.DeviceDescSC400Serial%=TwTouch_Device, MSY0101               ;Ser PnP SC 400/800
%TwTouch.DeviceDescSC500Serial%=TwTouch_Device, MSY0103               ;Ser PnP SC 500
%TwTouch.DeviceDescDSTSerial%=TwTouch_Device,   MSY0301               ;Ser PnP DST

;* These hardware IDs are for the USB HID controllers *
%TwTouch.DeviceDescSC400USB%=TwTouch_Device,    USB\VID_0596&PID_0100 ;USB SC 400/800
%TwTouch.DeviceDescSC500USB%=TwTouch_Device,    USB\VID_0596&PID_0102 ;USB SC 500
%TwTouch.DeviceDescDSTUSB%=TwTouch_Device,      USB\VID_0596&PID_0300 ;USB DST
%TwTouch.DeviceDescCX100%=TwTouch_Device,       USB\VID_0596&PID_0108 ;USB CX 100 Series

[Standard.NTamd64]

;* This is the pseudo device used by the non-PnP serial bus driver *
%TwTouch.DeviceDescSerial%=TwTouch_Device,	PnP\TwTouch	      ;Non-PnP Serial

;* These hardware IDs are for the EX II USB controllers *
%TwTouch.DeviceDescEXIIUSB%=TwTouch_Device,	USB\VID_0596&PID_0001 ;USB EXII
%TwTouch.DeviceDescEXIIUSBRom%=TwTouch_Device,	USB\VID_0596&PID_0002 ;USB EXII fix code
%TwTouch.DeviceDescEXIIHID%=TwTouch_Device,     USB\VID_0596&PID_0003 ;USB EXII HID

;* These hardware IDs are for the serial PnP controllers *
%TwTouch.DeviceDescSC400Serial%=TwTouch_Device, MSY0101               ;Ser PnP SC 400/800
%TwTouch.DeviceDescSC500Serial%=TwTouch_Device, MSY0103               ;Ser PnP SC 500
%TwTouch.DeviceDescDSTSerial%=TwTouch_Device,	MSY0301               ;Ser PnP DST

;* These hardware IDs are for the USB HID controllers *
%TwTouch.DeviceDescSC400USB%=TwTouch_Device,	USB\VID_0596&PID_0100 ;USB SC 400/800
%TwTouch.DeviceDescSC500USB%=TwTouch_Device,	USB\VID_0596&PID_0102 ;USB SC 500
%TwTouch.DeviceDescDSTUSB%=TwTouch_Device,	USB\VID_0596&PID_0300 ;USB DST
%TwTouch.DeviceDescCX100%=TwTouch_Device,       USB\VID_0596&PID_0400 ;USB CX 100 Series

; ***********************************************************************

[TwTouch_Device.NT]
include=msmouse.inf
CopyFiles=Drivers_Dir,mouclass_CopyFiles

[TwTouch_Device.ntamd64]
include=msmouse.inf
CopyFiles=Drivers_Dir,mouclass_CopyFiles

[TwTouch_Device.NT.Services]
AddService = TwTouch,%SPSVCINST_ASSOCSERVICE%, TwTouch_Service_Inst, TwTouch_Reg_Inst
include=msmouse.inf
needs=MouClass.Services

[TwTouch_Device.ntamd64.Services]
AddService = TwTouch,%SPSVCINST_ASSOCSERVICE%, TwTouch_Service_Inst, TwTouch_Reg_Inst
include=msmouse.inf
needs=MouClass.Services

[TwTouch_Service_Inst]
DisplayName    = %TwTouch.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\TwTouch.sys
LoadOrderGroup = Pointer Port

[TwTouch_Reg_Inst]
AddReg = TwTouch_AddReg

[TwTouch_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\TwTouch\Parameters,,,
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\TwTouch.sys"
HKR,,TypesSupported,0x00010001,7

[Drivers_Dir]
TwTouch.sys

; ***********************************************************************
[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
MMM = "3M"
StdMfg = "(3M devices)"
DiskId1 = "MT 7 Software Installation Media"
TwTouch.DeviceDescSerial = "MicroTouch Serial Touch Screen"
TwTouch.DeviceDescSC400Serial = "MicroTouch SC 400/800 Serial Touch Screen"
TwTouch.DeviceDescSC500Serial = "MicroTouch SC 500 Serial Touch Screen"
TwTouch.DeviceDescDSTSerial = "MicroTouch DST Serial Touch Screen"
TwTouch.DeviceDescEXIIUSB = "MicroTouch EX II USB Touch Screen"
TwTouch.DeviceDescEXIIUSBRom = "MicroTouch EX II USB ROM Touch Screen"
TwTouch.DeviceDescEXIIHID = "MicroTouch EX II HID Touch Screen"
TwTouch.DeviceDescCX100 = "MicroTouch CX 100 Series USB Touch Screen"
TwTouch.DeviceDescSC400USB = "MicroTouch SC 400/800 USB Touch Screen"
TwTouch.DeviceDescSC500USB = "MicroTouch SC 500 USB Touch Screen"
TwTouch.DeviceDescDSTUSB = "MicroTouch DST USB Touch Screen"
TwTouch.SVCDESC = "MicroTouch Touch Screen"
mouclass.SvcDesc = "Mouse Class Driver"
MouseClassName = "Mice and other pointing devices"
