#   Copyright (c) By Dialogue Technology Corp. All rights reserved.
#   03/01/2010
#############################################################################

PenMount USB Driver Package for Windows CE.Net 5.0

1. Copy PenMount to $(_WINCEROOT)\Public

2. Run Platform Builder. From menu, select Tools -> CEC Editors

3. From CEC Editors menu, select File -> Open 
   From the file dialog, select $(_WINCEROOT)\Public\PenMount\PMUsb\PM2Usb.cec 
   and click Open.
   From CEC Editors menu, select Catalog -> Add to Catalog

4. Return Platform Builder and right-click on the Catalog and select 
   "Refresh Catalog". 
   
5. Locate "Third Party\Device Drivers\Touch\PenMount USB". Then 
   right-click and select 'Add to OS Design'.

6. Please edit PM2USB.reg for hardware configuration. For example:
   
   "HalfSpeed"=dword:1        ; set "HalfSpeed" = 1 to slow-down the sample rate 
                              ; of PenMount 6000.

   "DisableEEPROM" = dword: 1 ; disable that storing calibrate data to EEPROM 
                              ; of controller.

   "NoCal16"=dword:0          ; "NoCal16" - remove 16-point calibrate option from UI.
   "DefaultCalib"=dword:9     ; "DefaultCalib" - setting defualt calibrate algorithm.
                              ; 0 --> Standard Calibrate
                              ; 4 --> Advanced  4-Points Calibrate
                              ; 9 --> Advanced  9-Points Calibrate
                              ; 10--> Advanced 16-Points Calibrate

   (PS: These registries is useless for PenMount 5000)
   (PS2: This driver can detect the controller (6000U or 5000). )


7. Build OS/Sysgen and Make Run-Time Image

8. [NOTE] When you got error after 6-step. Please execute prelink.bat in
   $(_WINCEROOT)\Public\PenMount\PMUsb\ . And do "Make Run-Time Image" from 
   menu.

