; Eric: It will use "Prefix" and "Index" for the device file name of 
; PenMount Serial driver.
;
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\PMSer]
   "Dll"="pmser.dll"   
   "Prefix"="PMT"
   "Index"=dword:2
   "Order"=dword:3
   "Port"=dword:1
;   "Protocol"=dword:1       ;PM9000
   "Protocol"=dword:3       ;PM6000R (Serial)
;   "Baudrate"=dword:2580   ; 9600
   "Baudrate"=dword:4B00    ; 19200
   "PMode"=dword:1
   "MinADX"=dword:0033
   "MinADY"=dword:0067
   "MaxADX"=dword:0378
   "MaxADY"=dword:03A9
;
;   "ActiveScreenRectLeft"   =dword:30
;   "ActiveScreenRectRight"  =dword:31F
;   "ActiveScreenRectTop"    =dword:30
;   "ActiveScreenRectBottom" =dword:257
;   "ActualScreenWidth"      =dword:320  ;800
;   "ActualScreenHeight"     =dword:258  ;600

; When DisableEEPROM = 1, It can disable EEPROM feature
;    "DisableEEPROM" = dword: 1


[HKEY_LOCAL_MACHINE\Software\PenMount\Calibrate]
    "NoCal16"=dword:0
;    "DefaultCalib"=dword:9

; "NoCal16" - remove 16-point calibrate option from UI.
; 1 -> remove
; 0 -> show 

; "DefaultCalib" - setting defualt calibrate algorithm.
; 0 --> Standard Calibrate
; 4 --> Advanced  4-Points Calibrate
; 9 --> Advanced  9-Points Calibrate
;10 --> Advanced 16-Points Calibrate
