HID touch screen driver installation for Fedora 5 and X11 
(C) 2008 AIM TOUCH TECHNOLOGY CO.,LTD.

==============================================================================
QUICKSTART GUIDE
==============================================================================
1. setup xfree driver
   a. decompress xfhiddrv_drv.tar.gz
      #gzip -d xfhiddrv_drv.tar.gz
      #tar xvf xfhiddrv_drv.tar 
   b. Copy xfhiddrv_drv.so to /usr/lib/xorg/modules/input/xfhiddrv_drv.so 

      #cp   xfhiddrv_drv.o /usr/lib/xorg/modules/input/xfhiddrv_drv.so
   c. Add the following lines into xorg.conf(maybe in /etc or /etc/X11)file.
   Set "ServerLayout"  section as the following.

    	InputDevice 	"HID TOUCH" 


   d. Add the a new "InputDevice" Section as the following.
Section "InputDevice"
        Identifier  "HID TOUCH"
        Driver      "xfhiddrv"
        Option      "Device" "/dev/ttyS0"
        Option      "ScreenNo" "0"
        Option      "Rotation" "0"
        Option      "SwapY" "0"
        Option      "DebugLevel" "0"
        Option      "AlwaysCore"
        Option      "UpSound" "1"
        Option      "DownSound" "1"
        Option      "AutoRightClick" "1"
        Option      "TouchMode" "2"
EndSection

    In the item of "Device", you must depend on your computer. So, it can be the value, 
such as the followings.
        USB DEVICE: "/dev/hiddevx"  x=0, 1, 2,..., n
        RS232 DEVICE:"/dev/ttySx"   x=0, 1, 2,..., n

   e. Press Ctrl+Alt+Backspace to restart X server. 

2. Setup and run Linear Utility:
   I. Linearity Utility:
   a. installation 
      step 1. decompress LinearAp.tar.gz 
         #gzip -d LinearAp.tar.gz
         #tar xvf LinearAp.tar.gz 
 
   b. Run linearity utility
      I. HID device
      #./LinearAp  /dev/hiddevx n
      II. RS232 device
      #./LinearAp  /dev/ttySx n

      where x=0,1,2...n, n = 4 or 9 <default>  
      
      
