# ===================== Drvier Version ============================= #
# =                                                                = #
# =        eGalax Touch driver for 32bit Linux kernel 2.4.x        = #
# =                                                                = #
# = Driver version: 3.05.5025-32b-k24                              = #
# = Module version: 3.05                                           = #
# = Utilty version: 3.02.4307                                      = #
# =                                    released date: 2011/02/25   = #
# =                                    support: touch_fae@eeti.com = #
# ======================== File List =============================== #

  egalax_drv.o
	X module for XFree86 4.x.
  eGalaxTouch
	Configuration utility for eGalax Touch touchscreen.

	The Xorg module and configuration utility both support
	RS232, PS/2 and USB interfaces at the same time.

  Guide/How to build module.pdf
	For more information about building a kernel module that
	support USB eGalax Touch touchscreen.
  Guide/Driver Guide.pdf
	For more information about eGalax Touch driver.

  TKCal/
	The command line calibration tool for eGalax Touch touchscreen.
	The user can do calibration without using eGalax Touch utility.

  USBSrc/
	The souce code of USB eGalax Touch kernel module.

# ================================================================== #
