; for "6000 USB"
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\5345_24576\Default\3\PenMount_USB_HID_Class_Driver]
   "Dll"="pmusb.dll"
   
; for "5000 USB"
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\5345_20480\Default\3\PenMount_USB_HID_Class_Driver]
   "Dll"="pmusb.dll"

; for "5000 USB"
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\4612_39320\Default\3\PenMount_USB_HID_Class_Driver]
   "Dll"="pmusb.dll"
   
[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\PenMount_USB_HID_Class_Driver]
   "Dll"="pmusb.dll"
   "Prefix"="PMT"
   "Index"=dword:2

; When DisableEEPROM = 1, It can disable EEPROM feature
;    "DisableEEPROM" = dword: 1

; For 6000 only, to slow down it's sample rate to half
;   "HalfSpeed"=dword:1

[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\PenMount_USB_HID_Class_Driver\0]
   "MinADX"=dword:0
   "MaxADX"=dword:000003FF
   "MinADY"=dword:0
   "MaxADY"=dword:000003FF
   "PMode"=dword:6

[HKEY_LOCAL_MACHINE\Software\PenMount\Calibrate]
    "NoCal16"=dword:0
;    "DefaultCalib"=dword:9

; "NoCal16" - remove 16-point calibrate option from UI.
; 1 -> remove
; 0 -> show 

; "DefaultCalib" - setting defualt calibrate algorithm.
; 0 --> Standard Calibrate
; 4 --> Advanced  4-Points Calibrate
; 9 --> Advanced  9-Points Calibrate
;10 --> Advanced 16-Points Calibrate
