1. copy fedora-11-xfhiddrv-0.0.1.tgz to home folder
2. double click "fedora-11-xfhiddrv-0.0.1.tgz" and select "extract".
3. sudo -s
   keyin your password
4. #cd /home/user/fedora-11-xfhiddrv-0.0.1
5. #sh setup.sh
6. restart your computer
7. calibration tool
   #LinearAp /dev/usb/hiddev0 9
    /dev/usb/hidev0 --> copy from /etc/X11/xorg.conf
    9 --> calibration point (4 or 9)
8. #TouchPanelKit
